**True Metrix Air Settings:**

1. If your True Metrix Air device is not in the off state, then make it so now, by holding down the power button (located on the top of the device, between the left and right buttons).
2. With your True Metrix Air device in the off state; press and hold the power button until you hear a chime.
3. To set the date/time: Cycle through the hours to set the Hour and AM-PM setting, by tapping either left, or right buttons, then tap the power button to lock it in. Repeat this step for Minutes, Month, Day, and Year.
4. To set the Bluetooth feature: Cycle through “Yes” and “No” when BLE is displayed on screen, then tap the power button to lock it in (“Yes” to turn it on, and “No” to turn it off).
5. To set the Event Tags: Please refer to the [True Metrix Air Owners Booklet.](http://share.secondopinion.net/Activate%20BLE/TrueMetrix-AIR-User-Manual.pdf)
6. To set Test Reminders: Please refer to the [True Metrix Air Owners Booklet](http://share.secondopinion.net/Activate%20BLE/TrueMetrix-AIR-User-Manual.pdf).
7. To Exit settings: Press and Hold the power button until the device goes into the off state.

**Set the Activate BLE app to use a specific True Metrix Air device:**

1. Open the Active BLE app.
2. Tap the Settings icon on the top left of the app.
3. Tap the “PAIR” button.
4. Tap the “PAIR DEVICE” button under “True Metrix Air”.
5. On the True Metrix Air device, tap and release the power button (located on the top of the device, between the left and right buttons).
6. On the Activate BLE App, you will be presented with a dialog box to input a PIN to pair with the True Metrix Air device.
	1. The PIN is the last 6 digits of the True Metrix Air serial number (you can find this on the back of the True Metrix Air device).
		1. As an example; if your True Metrix Air has a serial number of “TB2774453”, then the PIN is “774453”.
	2. If the PIN dialog box does not present itself, then you may need to enable your True Metrix Air’s Bluetooth feature (follow the instructions in “True Metrix Air Settings”.
7. You will notice the text under “True Metrix Air” has changed to “Pair successful! Tap pair to pair new device”. (You can verify that the device paired properly by finding its name in your mobile device’s Bluetooth settings.)
	1. Note: You will need to tap this button again for any other True Metrix Air device, which you would like to pair.
8. Tap the Back icon on the top left of the app, to go back to Settings, and then tap the Back icon again to go back to the main capture screen; You should now see True Metrix Air “Waiting/Searching”